
CM9760-KBD SERIES ENCLOSURE

TECHNICAL SPECIFICATIONS
SECURITY SYSTEM


DIVISION – LEVEL 1___ 28 ELECTRONIC SAFETY AND SECURITY
                                    

LEVEL 2___28 20 00 ELECTRONIC SURVEILLANCE

LEVEL 3___28 23 00 VIDEO SURVEILLANCE

LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
1 GENERAL

A. Equipment and materials used shall be standard components that are manufactured and available for purchase as standard replacement parts as long as the product is commercially available from the manufacturer.  
B. All manufactured products shall be thoroughly tested and proven in actual use.
C. All manufactured products shall include, at no additional cost, online support services and availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) for emergencies.
D. The manufacturer shall repair or replace without charge, manufactured products proven defective in material or workmanship for the stated warranty period from the date of shipment. 
2 PRODUCTS
2.1 KEYBOARD

A. The keyboard controller shall provide the main user interface to the matrix system and have control of all system functions, including auxiliary relays, receivers, camera/monitor switching, multiplexer screen functions, VCR controllers, and macro programming and operation. 

B. The keyboard controller shall provide the creation and recall of pan/tilt/zoom (PTZ) patterns, zones, zone labels, and presets.
C. Each keyboard operator shall have a specific, unique, user-programmable password assigned to prevent unauthorized use.
D. The keyboard controller shall provide two internal relays to activate local devices, such as video printers and VCRs.
E. The keyboard controller keyboard shall meet or exceed the following design and performance specifications.

1. Electrical Specifications
a. Input Voltage


100-240 VAC, 50/60 Hz

b. Operating Voltage


12 VDC

c. Power Consumption

10 W

d. Communication


RS-422, full duplex

e. Operating Distance 


(Direct Control) 4,000 ft (1,219 m) on 24 AWG 
wire 

f. Connectors 



2, 8-pin RJ-45 connectors (female) (RS-422 
serial ports)1, 4-pin RJ-45 connector (female) (RS-232 serial port) 2, 6-pin RJ-45 connectors (female): 1 relay port; 1 PC bus port for future expansion

g. Internal Relay Rating

1 A

2. General Specifications

a. Joystick



Proportional, vector-solving, variable speed with 
zoom 

b. Display



4-line, backlit LCD for programming and control

3. LCD Menu Display


8 multifunction keys to access programming 
icons and menus 

4. Definable Keys 

a. Numeric Keys 


10-key numeric keypad (0-9) plus 2 additional 
keys for camera (Cam) and monitor (Mon) selection

b. Specialty Keys

1. (T) “Turbo” 


Activates the high-speed mode of PTZ camera 
systems

2. Bwd/Fwd 


Initiates backward or forward camera 
sequencing of the next camera or the last camera

3. Run/Mac 


Initiates sequencing and calls preprogrammed 
macros

4. Rcl/Alt 



Recalls previously selected cameras and calls 
the next camera in the group

5. Prst/Lock


Calls a preset position scene and locks the 
currently displayed camera to the monitor

6. Lens Control Keys

3 keys provide control for cameras equipped 
with motorized zoom lenses and motorized pan and tilt units, as follows:

7. In/Out 



Zoom in and out

8. Open/Close


Open or close the iris (only available when the 
appropriate lens is fitted)

9. Near/Far


Focus near and far
5. Physical Specifications
a. Operating Temperature

32º to 120º F (0º to 49º C)

b. Dimensions


1. CM9760-KBD


7.80" D x 15.53" W x 3.30" H 
(19.81 x 39.45 x 8.38 cm)


2. CM9760-KBR


1.75" D x 19.00" W x 7.00" H 
(4.45 x 48.26 x 17.78 cm)

c. Unit Weight

1. CM9760-KBD


4.59 lb (2.08 kg)

2. CM9760-KBR


6.40 lb (2.90 kg)

6. Construction



Polyester resin reinforced with fiberglass

7. Finish

a. CM9760-KBD


White

b. CM9760-KBD-B


Black

c. CM9760-KBR


Black
8. Certifications

a. CE, Class B

b. UL Listed

c. UL Listed to Canadian safety standards

d. FCC, Class B


F. Warranty

1. 24 Months, parts and labor


G. Pelco Model Numbers
1. CM9760-KBD-US


Full-function desktop variable-speed keyboard; 
white finish; 100-240 VAC, 50/60 Hz; USA standard power cord
2. CM9760-KBD-AU


Full-function desktop variable-speed keyboard; 
white finish; 100-240 VAC, 50/60 Hz; Australia standard power cord
3. CM9760-KBD-EU


Full-function desktop variable-speed keyboard; 
white finish; 100-240 VAC, 50/60 Hz; European standard power cord
4. CM9760-KBD-UK


Full-function desktop variable-speed keyboard; 
white finish; 100-240 VAC, 50/60 Hz; UK standard power cord
5. CM9760-KBD-B-US


Full-function desktop variable-speed keyboard; 
black finish; 100-240 VAC, 50/60 Hz; USA standard power cord
6. CM9760-KBD-B-AU


Full-function desktop variable-speed keyboard; 
black finish; 100-240 VAC, 50/60 Hz; Australia standard power cord
7. CM9760-KBD-B-EU


Full-function desktop variable-speed keyboard; 
black finish; 100-240 VAC, 50/60 Hz; European standard power cord
8. CM9760-KBD-B-UK


Full-function desktop variable-speed keyboard; 
black finish; 100-240 VAC, 50/60 Hz; UK standard power cord
9. CM9760-KBR-US


Full-function 19-inch EIA rack mount keyboard 
(4 RUs); black finish; 100-240 VAC, 50/60 Hz; USA standard power cord
10. CM9760-KBR-AU


Full-function 19-inch EIA rack mount keyboard 
(4 RUs); black finish; 100-240 VAC, 50/60 Hz; Australia standard power cord
11. CM9760-KBR-EU


Full-function 19-inch EIA rack mount keyboard 
(4 RUs); black finish; 100-240 VAC, 50/60 Hz; European standard power cord
12. CM9760-KBR-UK


Full-function 19-inch EIA rack mount keyboard 
(4 RUs); black finish; 100-240 VAC, 50/60 Hz; UK standard power cord
